| PDM-IR SDK 3.0.2 PDM-IR SDK

Public Attributes | List of all members
Errors_u Union Reference

## Public Attributes
unsigned long | Errors
struct {
unsigned short LSB
unsigned short MiddleSB
unsigned short MSB
unsigned __pad0__: 8
} | ErrorsBytes_s
struct {
unsigned int EepromMcu: 1
unsigned int EepromFpga: 1
unsigned int EepromBackup: 1
unsigned int DacTrigger: 1
unsigned int DacVpol: 1
unsigned int AdcVpol: 1
unsigned int TempRH: 1
unsigned int SpadThreshold: 1
unsigned int DigpotPulser: 1
unsigned int AdcTec: 1
unsigned int DacTec: 1
unsigned int Mapping: 1
unsigned int MatchingMcuFpga: 1
unsigned int HoldOff: 1
unsigned int AdcMax10: 1
unsigned int PllMax10: 1
unsigned int TonMax10: 1
unsigned int InThreshold: 1
unsigned int AuxThreshold: 1
unsigned int MAX10_Outs: 1
unsigned int MAX10_Bus: 1
unsigned int MAX10_Delays: 1
unsigned int Ampi: 1
unsigned int Vpol: 1
unsigned __pad0__: 8
} | ErrorsBits_s

The documentation for this union was generated from the following file:

- PDM-IR_SDK.c