| PDM-IR SDK 3.0.2 PDM-IR SDK

ft_program_data Member List

This is the complete list of members for ft_program_data, including all inherited members.

ACDriveCurrentH (defined in ft_program_data) | ft_program_data |
ACSchmittInputH (defined in ft_program_data) | ft_program_data |
ACSlowSlewH (defined in ft_program_data) | ft_program_data |
ADDriveCurrentH (defined in ft_program_data) | ft_program_data |
ADriveCurrent (defined in ft_program_data) | ft_program_data |
ADSchmittInputH (defined in ft_program_data) | ft_program_data |
ADSlowSlewH (defined in ft_program_data) | ft_program_data |
AHDriveCurrent (defined in ft_program_data) | ft_program_data |
AHSchmittInput (defined in ft_program_data) | ft_program_data |
AHSlowSlew (defined in ft_program_data) | ft_program_data |
AIsHighCurrent (defined in ft_program_data) | ft_program_data |
AIsVCP (defined in ft_program_data) | ft_program_data |
AIsVCP7 (defined in ft_program_data) | ft_program_data |
AIsVCP8 (defined in ft_program_data) | ft_program_data |
ALDriveCurrent (defined in ft_program_data) | ft_program_data |
ALSchmittInput (defined in ft_program_data) | ft_program_data |
ALSlowSlew (defined in ft_program_data) | ft_program_data |
ARIIsTXDEN (defined in ft_program_data) | ft_program_data |
ASchmittInput (defined in ft_program_data) | ft_program_data |
ASlowSlew (defined in ft_program_data) | ft_program_data |
BDriveCurrent (defined in ft_program_data) | ft_program_data |
BHDriveCurrent (defined in ft_program_data) | ft_program_data |
BHSchmittInput (defined in ft_program_data) | ft_program_data |
BHSlowSlew (defined in ft_program_data) | ft_program_data |
BIsHighCurrent (defined in ft_program_data) | ft_program_data |
BIsVCP (defined in ft_program_data) | ft_program_data |
BIsVCP7 (defined in ft_program_data) | ft_program_data |
BIsVCP8 (defined in ft_program_data) | ft_program_data |
BLDriveCurrent (defined in ft_program_data) | ft_program_data |
BLSchmittInput (defined in ft_program_data) | ft_program_data |
BLSlowSlew (defined in ft_program_data) | ft_program_data |
BRIIsTXDEN (defined in ft_program_data) | ft_program_data |
BSchmittInput (defined in ft_program_data) | ft_program_data |
BSlowSlew (defined in ft_program_data) | ft_program_data |
Cbus0 (defined in ft_program_data) | ft_program_data |
Cbus0H (defined in ft_program_data) | ft_program_data |
Cbus1 (defined in ft_program_data) | ft_program_data |
Cbus1H (defined in ft_program_data) | ft_program_data |
Cbus2 (defined in ft_program_data) | ft_program_data |
Cbus2H (defined in ft_program_data) | ft_program_data |
Cbus3 (defined in ft_program_data) | ft_program_data |
Cbus3H (defined in ft_program_data) | ft_program_data |
Cbus4 (defined in ft_program_data) | ft_program_data |
Cbus4H (defined in ft_program_data) | ft_program_data |
Cbus5H (defined in ft_program_data) | ft_program_data |
Cbus6H (defined in ft_program_data) | ft_program_data |
Cbus7H (defined in ft_program_data) | ft_program_data |
Cbus8H (defined in ft_program_data) | ft_program_data |
Cbus9H (defined in ft_program_data) | ft_program_data |
CDriveCurrent (defined in ft_program_data) | ft_program_data |
CIsVCP8 (defined in ft_program_data) | ft_program_data |
CRIIsTXDEN (defined in ft_program_data) | ft_program_data |
CSchmittInput (defined in ft_program_data) | ft_program_data |
CSlowSlew (defined in ft_program_data) | ft_program_data |
DDriveCurrent (defined in ft_program_data) | ft_program_data |
Description (defined in ft_program_data) | ft_program_data |
DIsVCP8 (defined in ft_program_data) | ft_program_data |
DRIIsTXDEN (defined in ft_program_data) | ft_program_data |
DSchmittInput (defined in ft_program_data) | ft_program_data |
DSlowSlew (defined in ft_program_data) | ft_program_data |
EndpointSize (defined in ft_program_data) | ft_program_data |
FT1248CpolH (defined in ft_program_data) | ft_program_data |
FT1248FlowControlH (defined in ft_program_data) | ft_program_data |
FT1248LsbH (defined in ft_program_data) | ft_program_data |
HighDriveIOs (defined in ft_program_data) | ft_program_data |
IFAIsFastSer (defined in ft_program_data) | ft_program_data |
IFAIsFastSer7 (defined in ft_program_data) | ft_program_data |
IFAIsFifo (defined in ft_program_data) | ft_program_data |
IFAIsFifo7 (defined in ft_program_data) | ft_program_data |
IFAIsFifoTar (defined in ft_program_data) | ft_program_data |
IFAIsFifoTar7 (defined in ft_program_data) | ft_program_data |
IFBIsFastSer (defined in ft_program_data) | ft_program_data |
IFBIsFastSer7 (defined in ft_program_data) | ft_program_data |
IFBIsFifo (defined in ft_program_data) | ft_program_data |
IFBIsFifo7 (defined in ft_program_data) | ft_program_data |
IFBIsFifoTar (defined in ft_program_data) | ft_program_data |
IFBIsFifoTar7 (defined in ft_program_data) | ft_program_data |
InvertCTS (defined in ft_program_data) | ft_program_data |
InvertDCD (defined in ft_program_data) | ft_program_data |
InvertDSR (defined in ft_program_data) | ft_program_data |
InvertDTR (defined in ft_program_data) | ft_program_data |
InvertRI (defined in ft_program_data) | ft_program_data |
InvertRTS (defined in ft_program_data) | ft_program_data |
InvertRXD (defined in ft_program_data) | ft_program_data |
InvertTXD (defined in ft_program_data) | ft_program_data |
IsFastSerH (defined in ft_program_data) | ft_program_data |
IsFifoH (defined in ft_program_data) | ft_program_data |
IsFifoTarH (defined in ft_program_data) | ft_program_data |
IsFT1248H (defined in ft_program_data) | ft_program_data |
IsoIn (defined in ft_program_data) | ft_program_data |
IsoInA (defined in ft_program_data) | ft_program_data |
IsoInB (defined in ft_program_data) | ft_program_data |
IsoOut (defined in ft_program_data) | ft_program_data |
IsoOutA (defined in ft_program_data) | ft_program_data |
IsoOutB (defined in ft_program_data) | ft_program_data |
IsVCPH (defined in ft_program_data) | ft_program_data |
Manufacturer (defined in ft_program_data) | ft_program_data |
ManufacturerId (defined in ft_program_data) | ft_program_data |
MaxPower (defined in ft_program_data) | ft_program_data |
PnP (defined in ft_program_data) | ft_program_data |
PowerSaveEnable (defined in ft_program_data) | ft_program_data |
PowerSaveEnableH (defined in ft_program_data) | ft_program_data |
ProductId (defined in ft_program_data) | ft_program_data |
PullDownEnable (defined in ft_program_data) | ft_program_data |
PullDownEnable5 (defined in ft_program_data) | ft_program_data |
PullDownEnable7 (defined in ft_program_data) | ft_program_data |
PullDownEnable8 (defined in ft_program_data) | ft_program_data |
PullDownEnableH (defined in ft_program_data) | ft_program_data |
PullDownEnableR (defined in ft_program_data) | ft_program_data |
RemoteWakeup (defined in ft_program_data) | ft_program_data |
Rev4 (defined in ft_program_data) | ft_program_data |
Rev5 (defined in ft_program_data) | ft_program_data |
RIsD2XX (defined in ft_program_data) | ft_program_data |
SelfPowered (defined in ft_program_data) | ft_program_data |
SerialNumber (defined in ft_program_data) | ft_program_data |
SerNumEnable (defined in ft_program_data) | ft_program_data |
SerNumEnable5 (defined in ft_program_data) | ft_program_data |
SerNumEnable7 (defined in ft_program_data) | ft_program_data |
SerNumEnable8 (defined in ft_program_data) | ft_program_data |
SerNumEnableH (defined in ft_program_data) | ft_program_data |
SerNumEnableR (defined in ft_program_data) | ft_program_data |
Signature1 (defined in ft_program_data) | ft_program_data |
Signature2 (defined in ft_program_data) | ft_program_data |
USBVersion (defined in ft_program_data) | ft_program_data |
USBVersion5 (defined in ft_program_data) | ft_program_data |
USBVersionEnable (defined in ft_program_data) | ft_program_data |
USBVersionEnable5 (defined in ft_program_data) | ft_program_data |
UseExtOsc (defined in ft_program_data) | ft_program_data |
VendorId (defined in ft_program_data) | ft_program_data |
Version (defined in ft_program_data) | ft_program_data |