| PDM-IR SDK 3.0.2 PDM-IR SDK

Public Attributes | List of all members
ft_eeprom_x_series Struct Reference

## Public Attributes
FT_EEPROM_HEADER | common
UCHAR | ACSlowSlew
UCHAR | ACSchmittInput
UCHAR | ACDriveCurrent
UCHAR | ADSlowSlew
UCHAR | ADSchmittInput
UCHAR | ADDriveCurrent
UCHAR | Cbus0
UCHAR | Cbus1
UCHAR | Cbus2
UCHAR | Cbus3
UCHAR | Cbus4
UCHAR | Cbus5
UCHAR | Cbus6
UCHAR | InvertTXD
UCHAR | InvertRXD
UCHAR | InvertRTS
UCHAR | InvertCTS
UCHAR | InvertDTR
UCHAR | InvertDSR
UCHAR | InvertDCD
UCHAR | InvertRI
UCHAR | BCDEnable
UCHAR | BCDForceCbusPWREN
UCHAR | BCDDisableSleep
WORD | I2CSlaveAddress
DWORD | I2CDeviceId
UCHAR | I2CDisableSchmitt
UCHAR | FT1248Cpol
UCHAR | FT1248Lsb
UCHAR | FT1248FlowControl
UCHAR | RS485EchoSuppress
UCHAR | PowerSaveEnable
UCHAR | DriverType

The documentation for this struct was generated from the following file:

- ftd2xx.h